Yes

Yes

Yes

No

No

No

Send Message to Subscriber

If Shock Sensor Value > 50

Start

Wait 1 minute

Send location and Sensor Value to Online Database Storage

Get GPS location and read Shock Sensor output

GSM initialized?

Initialize GSM

GPS initialized?

Initialize GPS