SYSTEM FLOW CHART

Yes

Yes

Yes

No

No

No

Connected to Network?

Initialize Sensors

Get Humidity Value, Water Level Value and Water Flow Value

Send data to Online Cloud Storage

Wait for 1 minute

Is Water Level above 50 cm?

Send message to Subscriber

Connect to Network

Initialize Success?

Initialize GSM

Start